**Abstract**

**Introduction**

**Debate re: field capacity and wilting point**

**Methods**

**Results**

**Conclusion**

**References**

AGU style

Correcting temperature sensitivity of ECH2O soil moisture sensors

Doug Cobos and Colin Campbell, Decagon Devices

A data-driven method to remove temperature effects in TDR-measured soil water content at a Mongolian site. Minjiao Lu1,2, Jeewantinie Kapilaratne1

and Ichirow Kaihotsu3

Hydrological Research Letters 9(1), 8–13 (2015) DOI: 10.3178/hrl.9.8