**Processing techniques for soil moisture and matric potential data from**

**Dry Creek Experimental Watershed**

John Shuler, Boise State University

GEOS597: Computation in the Geosciences

Due: 12/9/2016

**Abstract**

Unsaturated zone processes have important implications for routing of precipitation to various watershed scale fluxes, including streamflow discharge, evapotranspiration and groundwater recharge [*Vereecken* *et al*, 2008].

**Introduction**

**Debate re: field capacity and wilting point**

**Methods**

Workflow diagram

Accuracy of sensors

**Data and Results**

**Conclusion**

**References**

Chandler, D., M. Seyfried, J. McNamara (2016), Inference of Soil Hydrologic Parameters from Electronic Soil Moisture Records. In review for *Hydrologic Processes*

Cobos, D. and C. Campbell, (2007) Correcting temperature sensitivity of ECH2O soil moisture sensors, Decagon Devices, Pullman, WA

Hillel, D. (1998) *Environmental Soil Physics*: *Fundamentals, Applications, and Environmental Considerations*, 1st Edition, Academic Press, Cambridge, MA

Lu, M., J. Kapilaratne and I. Kaihotsu (2015), A data-driven method to remove temperature effects in TDR-measured soil water content at a Mongolian site. *Hydrological Research Letters*, 9(1), 8–13 DOI: 10.3178/hrl.9.8

Vereecken, H., J.A. Huisman, H. Bogena, J. Vanderborght, J.A. Vrugt, J.W. Hopmans (2008),

On the value of soil moisture measurements in vadose zone hydrology: a review.

*Water Resour. Res*., 44 Art. Nb. W00D06